|  |
| --- |
| **How to use this BPIR summary**BPIR regulations do not prescribe any specific layout or formatting of required [disclosure information](https://bpir.nz/bpir-regulations-and-requirements/disclosure-information/). You may choose to take parts of this BPIR Ready summary and integrate it into your existing technical information, or you may choose to create a specific BPIR disclosure information document.To create a specific BPIR disclosure information document:1. Download the DOCX or copy the summary into your preferred document editor
2. Edit the relevant parts of the document where desired, such as:
	* Any content adjustments to the summary (e.g. add/remove clauses)
	* Replace the placeholder 'responsible person' information
	* Any layout alternations (e.g.removing the appendix and adding personal branding)
3. Export to your preferred format (e.g. PDF) and publish on your website

Note: the DOCX converter is in its beta phase. Should you encounter any issues, please [contact us](https://bpir.nz/how-it-works/contact/). |

## Marmox Shower NichesBPIR Declaration

Version: 1/9/23

#### Designated building product: Class 1

#### Declaration

Marmox New Zealand Ltd has provided this declaration to satisfy the provisions of Schedule 1(d) of the Building (Building Product Information Requirements) Regulations 2022.

#### Product/system

|  |  |
| --- | --- |
| **Name** | Marmox Shower Niches |
| **Line** | The Pre-fabricated and flat-packed Marmox Shower Niche provides a low-cost, easily installed and completely waterproof alternative for shower niche construction.  |
| **Identifier** | MNVP 330330 | MNVP 630330 | MNVP 930330 |

#### Description

The Marmox Shower Niche is made from an extruded polystyrene core coated on either side with a thin but robust layer of fibreglass reinforced polymer concrete. It is available in flat packs which can be easily assembled.

Intended use: It can be used to form a recess for toiletries within showers and other wet areas.

Sizes MNVP 330330 Size:330 x 330mm | MNVP 630330 Size: 630 x 330mm | MNVP 930330 Size:930 x 330mm

Features

1. Available in flat packs that can be easily assembled
2. Ready to waterproof and then tile
3. Lightweight and easy to work with
4. 12.5mm thick and fits wall cavities 86mm or deeper
5. Can be used to form a recess for toiletries within showers and other wet areas
6. Perfect for a DIY bathroom

#### Scope of use

Marmox Shower Niches are intended for use in showers and bathrooms. They are installed within the shower enclosure to provide a convenient and waterproof storage space for toiletries, bath essentials and other items.

#### Conditions of use

Marmox Shower Niches are available in flat packs that can be easily assembled.

WARNING: Do not use solvent based adhesives to assemble this product.

#### Relevant building code clauses

#### Contributions to compliance

As mentioned in the BRANZ appraisal, Marmox insulation products, if designed, used, installed and maintained in accordance with the statements and conditions of this Appraisal, will meet or contribute to meeting the following provisions of the NZBC:

Clause B2 Durability - Performance B2.3.1 [b] 15 years and B2.3.2. Marmox insulation boards meet this requirement as they are used as an underlay for waterproofing membranes, they will be durable for at least 15 years, provided the tiling and waterproofing systems are maintained to ensure the boards and fixings remain dry in services.

Clause F2 Hazardous Building Materials: Performance F2.3.1. Marmox Insulation boards meet this requirement.

#### Supporting documentation

The following additional documentation supports the above statements:

|  |  |  |
| --- | --- | --- |
| **Shower Niche Installation Instructions** |  | [https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https://marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-Installation-Instructions-2018.pdf](https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https%3A//marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-Installation-Instructions-2018.pdf) |
| **Drawing: Shower Niche - 330mm x 330mm** |  | [https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https://marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-330mm-x-330mm.pdf](https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https%3A//marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-330mm-x-330mm.pdf) |
| **Drawing: Shower Niche - 630mm x 330mm** |  | [https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https://marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-630mm-x-330mm.pdf](https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https%3A//marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-630mm-x-330mm.pdf) |
| **Drawing: Shower Niche - 930mm x 330mm** |  | [https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https://marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-930mm-x-330mm.pdf](https://chrome-extension://efaidnbmnnnibpcajpcglclefindmkaj/https%3A//marmox.co.nz/wp-content/uploads/2018/12/Shower-Niche-930mm-x-330mm.pdf) |

For further information supporting Marmox Shower Niches claims refer to our website.

#### Contact details

|  |  |
| --- | --- |
| **Manufacture location** | Overseas |
| **Legal and trading name of manufacturer** | Chemicals for Modern Building |
| **Legal and trading name of importer** | Marmox New Zealand Ltd |
| **Importer address for service** | 483A Rosebank Road, Rosebank Road, Avondale Auckland 1026 |
| **Importer website** | [marmox.co.nz](http://marmox.co.nz) |
| **Importer NZBN** | 9429035092377 |
| **Importer email** | info@marmox.co.nz |
| **Importer phone number** | 0800 627 669 |

#### Responsible person

As the responsible person as set out in Regulation 3, I confirm that the information supplied in this declaration is based on information supplied to the company as well as the company's own processes and is therefore to the best of my knowledge, correct.

I can also confirm that Marmox Shower Niches is not subject to a warning on ban under [s26 of the Building Act](https://www.legislation.govt.nz/act/public/2004/0072/latest/DLM306353.html).

Signed for and on behalf of **Marmox New Zealand Ltd:**

Your Signature

Your Name
YOUR POSITION
Month Year

**Marmox New Zealand Ltd**
483A Rosebank Road, Rosebank Road, Avondale Auckland 1026 New Zealand
0800 627 669 | [marmox.co.nz](http://marmox.co.nz)

## Appendix

|  |
| --- |
| Note: The below appendix includes information relating to BPIR Ready.Publishing this information is not a requirement under BPIR. Its inclusion here is to provide a reference for how this BPIR summary was generated as well as to help summary creators understand the performance clauses suggested by BPIR Ready. |

#### BPIR Ready selections

**Category:** Other (custom)

|  | **Yes** | **No** |
| --- | --- | --- |
| Use on access routes  |  | **×**  |
| Use in areas with floor surface fire obligations  |  | **×**  |
| Use in wet areas  |  | **×**  |
| Use in food preparation areas  |  | **×**  |
| Part of a system for acoustic performance  |  | **×**  |

#### Building code performance clauses