|  |
| --- |
| **How to use this BPIR summary**  BPIR regulations do not prescribe any specific layout or formatting of required [disclosure information](https://bpir.nz/bpir-regulations-and-requirements/disclosure-information). You may choose to take parts of this BPIR Ready summary and integrate it into your existing technical information, or you may choose to create a specific BPIR disclosure information document.  To create a specific BPIR disclosure information document:   1. Download the DOCX or copy the summary into your preferred document editor 2. Edit the relevant parts of the document where desired, such as:    * Any content adjustments to the summary (e.g. add/remove clauses)    * Replace the placeholder 'responsible person' information    * Any layout alternations (e.g.removing the appendix and adding personal branding) 3. Export to your preferred format (e.g. PDF) and publish on your website |

## Raymor Cove Tapware BPIR Declaration

Version: V1

#### Designated building product: Class 1

#### Declaration

MICO NEW ZEALAND LIMITED has provided this declaration to satisfy the provisions of Schedule 1(d) of the Building (Building Product Information Requirements) Regulations 2022.

#### Product/system

|  |  |
| --- | --- |
| **Name** | Raymor Cove Tapware |
| **Line** | Raymor Tapware |
| **Identifier** | (7)711698 (7)711700 (7)711703 (7)711704 (7)711706 (7)711710 (7)711711 (7)711697 (7)711699 (7)711705 (7)711707 |

#### Description

Raymor Cove tapware is a wall-mounted and bench-mounted tap depending on the configuration, manufactured from brass, has a continuous temperature valve and a variable flow rate head.

It is suitable for domestic use, and with mains pressure water supply systems.

Raymor Cove tapware is available in two finishes, chrome or black.

Raymor Cove tapware has indicators which show the relative temperature range (red for hot and blue for cold)

#### Scope of use

Please refer to the specification and installation sheet for this product.

#### Conditions of use

Must be installed by a New Zealand registered plumber. Must be installed in accordance with a design/installation manual. Please refer to the the installation instructions for maintenance or cleaning instructions.

#### Relevant building code clauses

**B2 Durability** — B2.3.1 (c)

**F2 Hazardous building materials** — F2.3.1

**G1 Personal Hygiene** — G1.3.2

**G12 Water Supplies** — G12.3.5

#### Contributions to compliance

B2.3.1(a) (ii) and (iii) and B2.3.2: Raymor Cove tapware has a 20 year warranty and a 2 year warranty on the colour. Refer to the specification sheet and installation requirements for further information.

F2.3.1: Raymor Cove is safe when handled. There are no requirements for this product in order to comply with Acceptable Solution F2/AS1, First Edition Amendment 3, 2017.

G1. Raymor Cove tapware is easy to access and clean where required. It is also compliant and compatible with fittings made to AS/NZS 3500 standards.

#### Supporting documentation

The following additional documentation supports the above statements:

None added

For further information supporting Raymor Cove Tapware claims refer to our website.

#### Contact details

|  |  |
| --- | --- |
| **Manufacture location** | Overseas |
| **Legal and trading name of manufacturer** | ZHEJIANG SUERDA SANITARY CO |
| **Legal and trading name of importer** | MICO NEW ZEALAND LIMITED |
| **Importer address for service** | Unit 3/1 Show Place  Christchurch 8024 |
| **Importer website** | [www.mico.co.nz](http://www.mico.co.nz) |
| **Importer NZBN** | 9429040952543 |
| **Importer email** | info@mico.co.nz |
| **Importer phone number** | 033381009 |

#### Responsible person

As the responsible person as set out in Regulation 3, I confirm that the information supplied in this declaration is based on information supplied to the company as well as the company's own processes and is therefore to the best of my knowledge, correct.

I can also confirm that Raymor Cove Tapware is not subject to a warning on ban under [s26 of the Building Act](https://www.legislation.govt.nz/act/public/2004/0072/latest/DLM306353.html).

Signed for and on behalf of **MICO NEW ZEALAND LIMITED:**

Your Signature

Your Name  
YOUR POSITION  
Month Year

**MICO NEW ZEALAND LIMITED**  
Unit 3/1 Show Place Christchurch 8024 New Zealand  
033381009 | [www.mico.co.nz](http://www.mico.co.nz)

## Appendix

|  |
| --- |
| Note: The below appendix includes information relating to BPIR Ready.  Publishing this information is not a requirement under BPIR. Its inclusion here is to provide a reference for how this BPIR summary was generated as well as to help summary creators understand the performance clauses suggested by BPIR Ready. |

#### BPIR Ready selections

**Category:** Sanitary fixtures and appliances [legacy category]

|  | **Yes** | **No** |
| --- | --- | --- |
| Suitable for Accessible facilities |  | **×** |
| Provision of hot water | **×** |  |

#### Building code performance clauses

#### B2 Durability

B2.3.1

*Building elements* must, with only normal maintenance, continue to satisfy the performance requirements of this code for the lesser of the *specified intended life* of the *building*, if stated, or:

* (c) 5 years if: the building elements (including services, linings, renewable protective coatings, and fixtures) are easy to access and replace, and failure of those building elements to comply with the building code would be easily detected during normal use of the building.

#### F2 Hazardous building materials

F2.3.1

The quantities of gas, liquid, radiation or solid particles emitted by materials used in the *construction* of *buildings*, shall not give rise to harmful concentrations at the surface of the material where the material is exposed, or in the atmosphere of any space.

#### G1 Personal Hygiene

G1.3.2

*Sanitary fixtures* shall be located, constructed and installed to:

1. facilitate *sanitation*,
2. avoid risk of food contamination,
3. avoid harbouring dirt or germs,
4. provide appropriate privacy,
5. avoid affecting occupants of adjacent spaces from the presence of unpleasant odours, accumulation of offensive matter, or other source of annoyance,
6. allow effective cleaning,
7. discharge to a plumbing and drainage system as required by Clause G13 Foul water when water-borne disposal is used, and
8. provide a healthy safe disposal system when non-water-borne disposal is used.

#### G12 Water Supplies

G12.3.5

*Sanitary fixtures* and *sanitary appliances* must be provided with hot water when intended to be used for

1. utensil washing; and
2. personal washing, showering, or bathing.