|  |
| --- |
| **How to use this BPIR summary**BPIR regulations do not prescribe any specific layout or formatting of required [disclosure information](https://bpir.nz/bpir-regulations-and-requirements/disclosure-information). You may choose to take parts of this BPIR Ready summary and integrate it into your existing technical information, or you may choose to create a specific BPIR disclosure information document.To create a specific BPIR disclosure information document:1. Download the DOCX or copy the summary into your preferred document editor
2. Edit the relevant parts of the document where desired, such as:
	* Any content adjustments to the summary (e.g. add/remove clauses)
	* Replace the placeholder 'responsible person' information
	* Any layout alternations (e.g.removing the appendix and adding personal branding)
3. Export to your preferred format (e.g. PDF) and publish on your website
 |

## Lamilay UnderlayBPIR Declaration

Version:

#### Designated building product: Class 1

#### Declaration

QEP, CO. NZ has provided this declaration to satisfy the provisions of Schedule 1(d) of the Building (Building Product Information Requirements) Regulations 2022.

#### Product/system

|  |  |
| --- | --- |
| **Name** | Lamilay Underlay |
| **Line** | Lamilay Underlay |
| **Identifier** | Lamilay Underlay |

#### Description

Flooring underlay suitable for all laminate and engineered floating floors over wood and concrete sub-floors.

#### Scope of use

Building type; Residential Wearability; suitability in normal household traffic areas.

#### Conditions of use

Self Adhesive backing. Ensure substrate is clean, dry, and level before installation.

#### Relevant building code clauses

#### Contributions to compliance

Building Regulations 1992 - Clause 2B-Durability Lamilay Underlay, with only normal maintenance, will continue to satisfy the performance requirements of Building Regulations for 10 years

#### Supporting documentation

The following additional documentation supports the above statements:

None added

For further information supporting Lamilay Underlay claims refer to our website.

#### Contact details

|  |  |
| --- | --- |
| **Manufacture location** | Overseas |
| **Legal and trading name of manufacturer** | China |
| **Legal and trading name of importer** | QEP, CO. NZ |
| **Importer address for service** | 6 Canaveral Drive Auckland 0632 |
| **Importer website** | <https://www.qep-aust.com.au/> |
| **Importer NZBN** |  |
| **Importer email** | nzoffice@qep.com |
| **Importer phone number** | 09 415 9700 |

#### Responsible person

As the responsible person as set out in Regulation 3, I confirm that the information supplied in this declaration is based on information supplied to the company as well as the company's own processes and is therefore to the best of my knowledge, correct.

I can confirm that Lamilay Underlay is subject to a warning on ban under [s26 of the Building Act](https://www.legislation.govt.nz/act/public/2004/0072/latest/DLM306353.html):

Signed for and on behalf of **QEP, CO. NZ:**

Your Signature

Your Name
YOUR POSITION
Month Year

**QEP, CO. NZ**
6 Canaveral Drive Auckland 0632 New Zealand
09 415 9700 | <https://www.qep-aust.com.au/>

## Appendix

|  |
| --- |
| Note: The below appendix includes information relating to BPIR Ready.Publishing this information is not a requirement under BPIR. Its inclusion here is to provide a reference for how this BPIR summary was generated as well as to help summary creators understand the performance clauses suggested by BPIR Ready. |

#### BPIR Ready selections

**Category:** Other (custom)

#### Building code performance clauses